Par Statistics
Total Non-vccgnd Signals=269
Total Non-vccgnd Design Pins=709
Total Non-vccgnd Conns=709
Total Non-vccgnd Timing Constrained Conns=601
Phase 1 CPU=7.6 sec
Phase 2 CPU=9.2 sec
Phase 3 CPU=10.2 sec
Phase 4 CPU=11.9 sec
Phase 5 CPU=12.8 sec
Phase 6 CPU=17.2 sec
Phase 7 CPU=20.4 sec
Phase 8 CPU=20.4 sec
Phase 9 CPU=20.4 sec
Phase 10 CPU=20.5 sec
AvgWirelenPerPin Fanout 1=2.0
AvgWirelenPerPin Fanout 2=3.5
AvgWirelenPerPin Fanout 3=7.7
AvgWirelenPerPin Fanout 4=12.0
AvgWirelenPerPin Fanout 10=7.2
AvgWirelenPerPin Fanout 50=5.4
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0271