Par Statistics
Total Non-vccgnd Signals=16891
Total Non-vccgnd Design Pins=64680
Total Non-vccgnd Conns=64680
Total Non-vccgnd Timing Constrained Conns=53483
Phase 1 CPU=15.2 sec
Phase 2 CPU=22.2 sec
Phase 3 CPU=48.7 sec
Phase 4 CPU=57.0 sec
Phase 5 CPU=88.5 sec
Phase 6 CPU=94.3 sec
Phase 7 CPU=240.2 sec
Phase 8 CPU=240.2 sec
Phase 9 CPU=809.7 sec
Phase 10 CPU=812.3 sec
AvgWirelenPerPin Fanout 1=5.0
AvgWirelenPerPin Fanout 2=4.5
AvgWirelenPerPin Fanout 3=4.7
AvgWirelenPerPin Fanout 4=4.8
AvgWirelenPerPin Fanout 10=4.9
AvgWirelenPerPin Fanout 50=4.3
AvgWirelenPerPin Fanout 100=10.9
AvgWirelenPerPin Fanout 500=11.0
AvgWirelenPerPin Fanout 5000=10.8
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=2.2971