Par Statistics
Total Non-vccgnd Signals=4160
Total Non-vccgnd Design Pins=12852
Total Non-vccgnd Conns=12852
Total Non-vccgnd Timing Constrained Conns=11235
Phase 1 CPU=10.7 sec
Phase 2 CPU=13.8 sec
Phase 3 CPU=22.1 sec
Phase 4 CPU=26.5 sec
Phase 5 CPU=36.0 sec
Phase 6 CPU=36.0 sec
Phase 7 CPU=36.0 sec
Phase 8 CPU=36.0 sec
Phase 9 CPU=36.2 sec
Phase 10 CPU=36.8 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=4.0
AvgWirelenPerPin Fanout 3=3.7
AvgWirelenPerPin Fanout 4=4.8
AvgWirelenPerPin Fanout 10=3.9
AvgWirelenPerPin Fanout 50=4.3
AvgWirelenPerPin Fanout 100=10.8
AvgWirelenPerPin Fanout 500=3.8
AvgWirelenPerPin Fanout 5000=4.4
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3621