Par Statistics
Total Non-vccgnd Signals=4194
Total Non-vccgnd Design Pins=13402
Total Non-vccgnd Conns=13402
Total Non-vccgnd Timing Constrained Conns=11613
Phase 1 CPU=10.4 sec
Phase 2 CPU=13.6 sec
Phase 3 CPU=21.4 sec
Phase 4 CPU=25.5 sec
Phase 5 CPU=33.9 sec
Phase 6 CPU=33.9 sec
Phase 7 CPU=33.9 sec
Phase 8 CPU=33.9 sec
Phase 9 CPU=34.1 sec
Phase 10 CPU=34.8 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=2.5
AvgWirelenPerPin Fanout 3=2.7
AvgWirelenPerPin Fanout 4=3.8
AvgWirelenPerPin Fanout 10=4.4
AvgWirelenPerPin Fanout 50=3.7
AvgWirelenPerPin Fanout 100=10.4
AvgWirelenPerPin Fanout 500=3.9
AvgWirelenPerPin Fanout 5000=4.2
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3787