Par Statistics
Total Non-vccgnd Signals=5256
Total Non-vccgnd Design Pins=17219
Total Non-vccgnd Conns=17219
Total Non-vccgnd Timing Constrained Conns=15160
Phase 1 CPU=11.0 sec
Phase 2 CPU=15.9 sec
Phase 3 CPU=26.7 sec
Phase 4 CPU=31.8 sec
Phase 5 CPU=44.3 sec
Phase 6 CPU=45.6 sec
Phase 7 CPU=83.5 sec
Phase 8 CPU=83.5 sec
Phase 9 CPU=83.8 sec
Phase 10 CPU=84.7 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=4.5
AvgWirelenPerPin Fanout 3=3.3
AvgWirelenPerPin Fanout 4=3.0
AvgWirelenPerPin Fanout 10=6.1
AvgWirelenPerPin Fanout 50=4.1
AvgWirelenPerPin Fanout 100=10.1
AvgWirelenPerPin Fanout 500=4.9
AvgWirelenPerPin Fanout 5000=3.8
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.4820