Par Statistics
Total Non-vccgnd Signals=4194
Total Non-vccgnd Design Pins=13434
Total Non-vccgnd Conns=13434
Total Non-vccgnd Timing Constrained Conns=11634
Phase 1 CPU=10.5 sec
Phase 2 CPU=13.7 sec
Phase 3 CPU=22.4 sec
Phase 4 CPU=26.8 sec
Phase 5 CPU=34.9 sec
Phase 6 CPU=35.6 sec
Phase 7 CPU=35.6 sec
Phase 8 CPU=35.6 sec
Phase 9 CPU=35.9 sec
Phase 10 CPU=36.5 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=3.0
AvgWirelenPerPin Fanout 3=2.7
AvgWirelenPerPin Fanout 4=4.3
AvgWirelenPerPin Fanout 10=5.0
AvgWirelenPerPin Fanout 50=4.0
AvgWirelenPerPin Fanout 100=11.9
AvgWirelenPerPin Fanout 500=5.3
AvgWirelenPerPin Fanout 5000=5.1
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3466