Par Statistics
Total Non-vccgnd Signals=16888
Total Non-vccgnd Design Pins=64520
Total Non-vccgnd Conns=64520
Total Non-vccgnd Timing Constrained Conns=53380
Phase 1 CPU=15.4 sec
Phase 2 CPU=22.5 sec
Phase 3 CPU=46.0 sec
Phase 4 CPU=55.8 sec
Phase 5 CPU=85.7 sec
Phase 6 CPU=93.6 sec
Phase 7 CPU=152.2 sec
Phase 8 CPU=152.2 sec
Phase 9 CPU=154.9 sec
Phase 10 CPU=157.6 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=3.5
AvgWirelenPerPin Fanout 3=3.7
AvgWirelenPerPin Fanout 4=4.0
AvgWirelenPerPin Fanout 10=4.3
AvgWirelenPerPin Fanout 50=3.7
AvgWirelenPerPin Fanout 100=9.1
AvgWirelenPerPin Fanout 500=10.1
AvgWirelenPerPin Fanout 5000=9.4
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=2.5330