Par Statistics
Total Non-vccgnd Signals=4125
Total Non-vccgnd Design Pins=13142
Total Non-vccgnd Conns=13142
Total Non-vccgnd Timing Constrained Conns=11377
Phase 1 CPU=9.6 sec
Phase 2 CPU=12.4 sec
Phase 3 CPU=18.3 sec
Phase 4 CPU=22.2 sec
Phase 5 CPU=30.0 sec
Phase 6 CPU=30.0 sec
Phase 7 CPU=30.0 sec
Phase 8 CPU=30.0 sec
Phase 9 CPU=30.1 sec
Phase 10 CPU=30.7 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=2.5
AvgWirelenPerPin Fanout 3=3.0
AvgWirelenPerPin Fanout 4=3.8
AvgWirelenPerPin Fanout 10=4.4
AvgWirelenPerPin Fanout 50=3.7
AvgWirelenPerPin Fanout 100=10.0
AvgWirelenPerPin Fanout 500=3.9
AvgWirelenPerPin Fanout 5000=4.5
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3588