Par Statistics
Total Non-vccgnd Signals=4982
Total Non-vccgnd Design Pins=16167
Total Non-vccgnd Conns=16167
Total Non-vccgnd Timing Constrained Conns=13923
Phase 1 CPU=9.7 sec
Phase 2 CPU=12.5 sec
Phase 3 CPU=20.9 sec
Phase 4 CPU=24.9 sec
Phase 5 CPU=34.7 sec
Phase 6 CPU=34.7 sec
Phase 7 CPU=34.7 sec
Phase 8 CPU=34.7 sec
Phase 9 CPU=35.0 sec
Phase 10 CPU=35.8 sec
AvgWirelenPerPin Fanout 1=8.0
AvgWirelenPerPin Fanout 2=4.0
AvgWirelenPerPin Fanout 3=5.7
AvgWirelenPerPin Fanout 4=4.3
AvgWirelenPerPin Fanout 10=5.4
AvgWirelenPerPin Fanout 50=10.3
AvgWirelenPerPin Fanout 100=19.7
AvgWirelenPerPin Fanout 500=13.2
AvgWirelenPerPin Fanout 5000=4.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3558