Par Statistics
Total Non-vccgnd Signals=4583
Total Non-vccgnd Design Pins=14614
Total Non-vccgnd Conns=14614
Total Non-vccgnd Timing Constrained Conns=12565
Phase 1 CPU=10.6 sec
Phase 2 CPU=14.5 sec
Phase 3 CPU=23.9 sec
Phase 4 CPU=28.4 sec
Phase 5 CPU=37.5 sec
Phase 6 CPU=37.5 sec
Phase 7 CPU=37.5 sec
Phase 8 CPU=37.5 sec
Phase 9 CPU=37.8 sec
Phase 10 CPU=38.5 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=4.0
AvgWirelenPerPin Fanout 3=3.3
AvgWirelenPerPin Fanout 4=5.0
AvgWirelenPerPin Fanout 10=5.4
AvgWirelenPerPin Fanout 50=4.7
AvgWirelenPerPin Fanout 100=13.8
AvgWirelenPerPin Fanout 500=6.1
AvgWirelenPerPin Fanout 5000=5.1
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.2906