Par Statistics
Total Non-vccgnd Signals=4053
Total Non-vccgnd Design Pins=12830
Total Non-vccgnd Conns=12830
Total Non-vccgnd Timing Constrained Conns=11190
Phase 1 CPU=10.8 sec
Phase 2 CPU=13.8 sec
Phase 3 CPU=22.1 sec
Phase 4 CPU=26.3 sec
Phase 5 CPU=33.6 sec
Phase 6 CPU=33.6 sec
Phase 7 CPU=33.6 sec
Phase 8 CPU=33.6 sec
Phase 9 CPU=33.8 sec
Phase 10 CPU=34.4 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=3.0
AvgWirelenPerPin Fanout 3=2.7
AvgWirelenPerPin Fanout 4=4.5
AvgWirelenPerPin Fanout 10=4.6
AvgWirelenPerPin Fanout 50=4.5
AvgWirelenPerPin Fanout 100=5.8
AvgWirelenPerPin Fanout 500=4.2
AvgWirelenPerPin Fanout 5000=4.7
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3233