Par Statistics
Total Non-vccgnd Signals=5472
Total Non-vccgnd Design Pins=16502
Total Non-vccgnd Conns=16502
Total Non-vccgnd Timing Constrained Conns=14025
Phase 1 CPU=10.3 sec
Phase 2 CPU=14.8 sec
Phase 3 CPU=25.0 sec
Phase 4 CPU=28.9 sec
Phase 5 CPU=38.4 sec
Phase 6 CPU=38.4 sec
Phase 7 CPU=38.4 sec
Phase 8 CPU=38.4 sec
Phase 9 CPU=38.4 sec
Phase 10 CPU=39.1 sec
AvgWirelenPerPin Fanout 1=6.0
AvgWirelenPerPin Fanout 2=4.0
AvgWirelenPerPin Fanout 3=3.0
AvgWirelenPerPin Fanout 4=4.5
AvgWirelenPerPin Fanout 10=5.0
AvgWirelenPerPin Fanout 50=5.1
AvgWirelenPerPin Fanout 100=10.4
AvgWirelenPerPin Fanout 500=5.4
AvgWirelenPerPin Fanout 5000=3.6
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.3616